From ef1b0370f33a69ef2e61635ba82ef23228c8fb1f Mon Sep 17 00:00:00 2001
From: Ren Yu <yux.ren@intel.com>
Date: Fri, 24 May 2019 14:55:10 +0800
Subject: [PATCH] Add the pre-timeout interrupt defined in IPMI spec

The IPMI watchdog pre-timeout interrupt is used to set the different
pre-timeout interrupt source. Add them as a dbus property,
IPMI set/get watchdog commands will use it.

Signed-off-by: Ren Yu <yux.ren@intel.com>
Upstream-Status: Pending
---
 .../State/Watchdog.interface.yaml             | 22 +++++++++++++++++++
 1 file changed, 22 insertions(+)

diff --git a/yaml/xyz/openbmc_project/State/Watchdog.interface.yaml b/yaml/xyz/openbmc_project/State/Watchdog.interface.yaml
index 556dca1..dbca599 100644
--- a/yaml/xyz/openbmc_project/State/Watchdog.interface.yaml
+++ b/yaml/xyz/openbmc_project/State/Watchdog.interface.yaml
@@ -33,6 +33,11 @@ properties:
       description: >
           The action the watchdog should perform when it expires.
       default: "HardReset"
+    - name: PreTimeoutInterrupt
+      type: enum[self.PreTimeoutInterruptAction]
+      description: >
+          The BMC generates the selected interrupt before the timer expires.
+      default: "None"
     - name: Interval
       type: uint64
       description: >
@@ -73,6 +78,23 @@ enumerations:
             description: >
                 Perform a power cycle of the system.
 
+    - name: PreTimeoutInterruptAction
+      description: >
+          The type of PreTimeout Interrupt.
+      values:
+          - name: "None"
+            description: >
+                Do nothing.
+          - name: "SMI"
+            description: >
+                SMI.
+          - name: "NMI"
+            description: >
+                NMI / Diagnostic Interrupt.
+          - name: "MI"
+            description: >
+                Messaging Interrupt.
+
     - name: TimerUse
       description: >
           The type of timer use.
-- 
2.25.1

