From d486099eb09eee64a0e1dc45785785f22c61a4a8 Mon Sep 17 00:00:00 2001
From: wangjue <jue.wang2@luxshare-ict.com>
Date: Tue, 24 Dec 2024 16:52:19 +0800
Subject: [PATCH] Set Available to false when dimm temp reading is not ready

Signed-off-by: wangjue <jue.wang2@luxshare-ict.com>
---
 src/DIMMTempSensor.cpp | 1 +
 1 file changed, 1 insertion(+)

diff --git a/src/DIMMTempSensor.cpp b/src/DIMMTempSensor.cpp
index 7c4412f..a0c9d76 100644
--- a/src/DIMMTempSensor.cpp
+++ b/src/DIMMTempSensor.cpp
@@ -247,6 +247,7 @@ void DIMMTempSensor::read(const std::string& sensorName)
         }
         else
         {
+            markAvailable(false);
             updateValue(std::numeric_limits<double>::quiet_NaN());
         }
         read(sensorName);
-- 
2.34.1

